---------------------------------------------------------------------------
-----			                   WELCOME!!!!                        -----
-----                                                                 -----
-----                     ANY QUESTIONS OR CONCERNS???                -----
-----              CONTACT JJ ROBERTS OR HAMISH AHERN ON FACEBOOK!    -----
-----             CAN EASILY BE FOUND WITHIN EVOSCAN FACEBOOK GROUP!  -----
-----                -------------------------------------            -----
-----							    CREATOR :                         -----
-----                      JJ ROBERTS aka ALPHATUNE101                -----
-----                   WATCH FOR EVOSCAN WEBSITE FOR UPDATES!        -----
-----                SAME PURCHASED SERIAL KEY WILL STAY VAILID!      -----
---------------------------------------------------------------------------


NOTES : 

1. Auto Vehicle Selection Will Determine Base On RomID ( Select Unknown_ID If ROM_ID Isn't Listed! )

2. This Software Does Carry a "Auto-Save" Feature. Be Assure To Create Back-Up Of Stock File!

3. Sharing Paid License ( IS NOT ) Being Tolerated. If Any Recordings,
Your License Will Be Revoked! 

4. There Is ( NO REFUND ) Within This Software. Once Email Is Sent With License. 



// ** AI Model Instructions ** \\

NOTE : Please Move The "Models" Folder Directly To Your "EvoPro ROM Tool v3.58" Folder, Unfortunately Was To Large To Package All Into Installer... 

URL : https://drive.google.com/file/d/1ZHkrHfciDmDe7S5SUZJHge6FIh5k2bA7/view?usp=drive_link




// ** Mode-23 XML Instructions ** \\

1. Must Be Working On a Vehicle Within The Years 768KB-2014 Vehicles! Outlander/Lancer Base Model/EvoX/RA/Etc... All Available.

2. Inject Binary File Inside of EvoPro, And Select Proper RomID. Select UnknownID If Not Listed, and Select Your Correct Vehicle.

3. Inside Of Quick Command #1, You Will Need To Enable RAM Access Patch ( Mode23 ) For Your Vehicle.

4. Inside Of Mode-23 XML Generator, You Can Select All, or Optional Data Paramaters.

5. Click Generate, and Save To Forwarded Directory. Once Completed Save a Copy and Move Inside ( Documents -> EvoScan - > DataSettings )

6. Open Inside Evoscan, and Click Onto All Of The CheckBoxes and Turn Your Vehicle On With The Tactrix Cable Connected To Your Vehicle. Time To Start Data Logging!
